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1. Dimensions/Volume/Weight
	Diameter
	148 mm

	Height
	263mm

	Volume
	3.2 L

	Weight (empty keg)
	0.21 kg


2. Materials
	Inner bag
	9 layers laminate, Multi layers high barrier

	Valve
	PA (food grade)

	Spear housing
	PA (food grade)

	Springs (food contact)
	Stainless Steel 304

	Springs (non food contact)
	Stainless Steel 304

	Seals
	TPE (food grade)

	Keg
	PET

	Others
	PP


3. Shelf life and barrier performance
	Filled keg
	Depends on filled beverage, up to 12 months

	O₂ pick up per year
	< 0.8 ppm

	CO₂ loss per year
	<10% (carbonization: 5.5g/L)

	Sealing of spear/inner bag
	≥6 bar, free of leakage

	Sealing of spear and keg
	≥6 bar, free of leakage

	Sealing of valve from outside
	≥2 bar, free of leakage

	Sealing of spear and metal coupler
	≥2 bar, free of leakage


4. Mechanical/physical Properties
	Operation temperature
	0°C ~ 35°C

	Maximum dispense pressure
	2 bar

	Strength at break
	≥8 bar, free of burst into pieces

	safety strength
	≥3 bar

	Impact and stress concentration
	No piercing, scratch mark on the kegs are allowed.

	Handle strength
	≥1 hour, no crack on handle of keg full filled.

	Strain strength
	≥8 bar, free of leakage of the keg body.

	Connection strength
	≥6 bar, no shooting out and/or damage of spear head.

	Maximum force loading on spear
	≥50 kg

	Disposal
	The Gprokeg is designed to give an extreme low impact on the environment, the empty keg is 100% recyclable, the product is 100% compliant to the EU Directive 94/62/EC



5. keg coupler type
	Specific coupler fit with Gprokeg specific dispensing/filling tool
	


6. Food contact and microorganism
	Food contact approval
	All materials and additives used for the components intent to contact with food  comply with European regulation EU10/2011 and other regulations

	FDA
	All materials and additives used for the components intent to contact with food  comply with FDA cfr 175.300

	Flavor/taste stability
	All materials intent to contact with beverages are free of small molecular migration and free of chemical reaction with content of beverages, keeping flavor/taste stability of beverages.

	total numbers of colony for spear and inner bag
	0

	total numbers of Bacillus coli in spear and inner bag
	0


7. Filling and Dispensing
	Filling volume
	≥5.0 liters, beer temperature: 0°C ~ 3°C； filling pressure: 2.0bar

	beer dispensing
	Foam height: 10mm~30mm, beer temperature: 3°C; dispensing pressure:  1bar


8. Palletizing
Empty keg
	Pallet size
	1200x1000x110mm, one-way

	Carton box size
	610x310x290mm

	Kegs per carton box
	8

	Carton box per pallet
	48

	Kegs per pallet
	384

	Orientation
	Upside up

	Height
	2.43m (for HC container)

	Weight
	106kg

	Pallets are wrapped with stretch film



Filled keg
	Pallet size
	1200x1000x110mm, one-way

	Carton box size
	610x310x290mm

	Kegs per carton box
	8

	Carton box per pallet
	48

	Kegs per pallet
	384

	Orientation
	Upside up

	Height
	2.43m (for HC container)

	Max. layers in warehouse
	10
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