[image: ]Technical Specification
Portable dispensing tool for party keg

1. [image: ]Dimensions/Weight
	Length
	169 mm

	Width
	72mm

	Height
	136mm

	Weight (empty bag)
	0.28 kg


2. Materials
	Dispense Tube
	HDPE

	Pump housing
	PC/ABS

	Others
	POM


3. Mechanical/physical Properties
	Operation temperature
	0°C ~ 45°C

	Working pressure
	0.5bar(7.25psi) ~ 1.0 bar (14.5psi)

	Battery
	Lithium ion battery, 3.7V, 1100mAh

	Maximum beer flow rate
	≥1.5L/min

	Foam level
	10mm ~ 30mm (adjustable)


4. Food contact
	EU food contact approval
	All materials and additives used for the components intent to contact with food  comply with European regulation EU10/2011

	FDA
	All materials and additives used for the components intent to contact with food  comply with FDA cfr 175.300


5. Packaging
	Box size
(mm)
	Carton size
(mm)
	Qty 
(pcs)
	Net Weight
(kg)
	Gross Weight
(kg)

	118 (L) x 75 (W) x 140 (H)
	480 (L) x 450 (W) x 310 (H)
	48
	13.5
	14.3
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